PRINTING CALIBRATION

Galileo Scale Model

PARTS SHEET 2: HGA Reflector & Sun Shades PRINT ON HEAVY WHITE PAPER

BUS SUNSHADE BOTTOM

HGA SUNSHADE TOP HGA SUNSHADE BOTTOM

REFLECTOR STRUCTURE FRONT BACK

Galileo’s path through the inner solar system, needed for gravity assist early in its flight to gain enough energy to reach Jupiter, required the installation of sunshades to protect the HGA, the spacecraft bus, and many other parts of the spacecraft, from the Sun’s heat. A second low-gain antenna was mounted on an RTG boom for telecommunications. Low-Gain Antenna No. 1 (LGA-1), shown atop the HGA SUNSHADE, supports communications with Earth since the HGA is unusable.

CUT PARTS AWAY FROM AREAS MARKED WITH THIS SHADING (APPEARS BLUE ON A COLOR MONITOR, AND GREY ON A B&W PRINTER)

FOR ILLUSTRATED ASSEMBLY INSTRUCTIONS, GO TO http://www.jpl.nasa.gov/galileo/model

BUS SUNSHADE TOP

(Do not cut white circle)

LGA-1